For 18V and high current load, thermal calculations are following

As can be seen from the figure x, thermal calculations are approximately equal to measured/observed temperature values.